

**KT1SU Temperature Logger Instructions (Single Use)**

**Important information before use - WARNING:**  
The **KT1SU** is a **single-use temperature logger**. This means it can only be **started once**. Once activated, it cannot be restarted or reprogrammed.

**Pre-configured**

This logger has been **pre-programmed** by us. You do not need to configure any settings.

**Starting the logger**

1. Press and hold the **start button** for approximately **8 seconds**.
2. The logger is activated when **all LEDs flash up and down**.
   * If the LEDs do not flash, the logger may have already been started or the button was not held long enough.

**After use – reading out the logger**

1. Plug the logger into a **USB port on your computer** after transport.
2. The logger will behave like a USB stick and automatically generate:
   * A **PDF report**
   * Optionally, additional files such as .TXT, .CSV or .KLG

**Calibration certificate**

You can find the link to the **individual calibration certificate**:

* In the **PDF report** generated by the logger
* Or via the **KeyTag Manager Software** during data download

**Software requirement**

Always use the **latest version** of the **KeyTag Manager software**:

* Version **1.19.10** or higher
* Download at: [www.dataloggers.shop/Software](https://www.dataloggers.shop/Software)

**Support and contact**

Do you have questions or need assistance with your KT1SU logger?  
We are happy to help.

**Dataloggers.shop**  
[www.dataloggers.shop](http://www.dataloggers.shop)  
✉ mail@tempro.be